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Groundwater and Water Supply: desk report
Tamsin Ridge Solar and Storage
This is a fictional demonstration project in which every organisation, person, parcel and finding is invented.
One row of the risk matrix, AQ-03 Groundwater and Water Supply, in the Aquatic Resources section: what the record holds on it.
A desk review of the record as it stood: not a field survey and not a modelled study.
	Information cut-off
	2023-08-01

	Row in the matrix
	AQ-03 Groundwater and Water Supply


1 Finding
1  Resource is present within area, impact unlikely
up to 2  Impacts likely but may be easily resolved
The engine shows this rating as 1-2
	The rule
	Code computed the rating from the assessor's inputs:
present, impact unlikely -> 1
Set by the rule

	Decision
	Released with flags

	The engine's reasons
	Agencies not in the register or the evidence: Carroll County, SFM
Independent assessments split on the category (5 samples: {'2': 1, '1': 4})

	Evidence state
	REPORTED · desktop, consultant or developer record


The assessor's comments
Nearby residences and farmsteads rely on private wells in the shale and sandstone aquifer. Ohio EPA mapping shows no source water protection area within the parcels. No fire hydrants in the area; nearest pressurized water is in Carrollton, about 4 miles away. No well survey is in the data room.
Worst case
If what is pending at the cut-off went badly, the same rule gives a higher rating.
	Scenario
	The survey finds private wells within pile-driving offsets, or the BESS needs a new on-site well, so testing and restricted methods remain likely.

	Step still pending
	Private well survey and fire water supply decision

	Inputs in the worst case
	Extent peripheral · Avoidable partly · Pathway standard · Impact likely yes

	The rule on the worst case
	worst case: impact_likely=yes -> 2

	Claims that make it plausible
	C-ae204b1b36, C-5a262c9439, C-04a3f6e338


2 What the record shows
The five inputs
Present: yes
Nearby residences and farmsteads rely on private wells in the shale and sandstone aquifer (C-ae204b1b36). Ohio EPA mapping shows no source water protection area within the parcels (C-afa9ffa993), which does not conflict: private wells are nearby, not protection areas. No hydrants exist and the nearest pressurized water is about 4 miles away (C-04a3f6e338), so fire water will need tanks or hauling.
Cites C-ae204b1b36, C-afa9ffa993, C-04a3f6e338
Extent: peripheral
Private wells are described as nearby, and no protection area lies within the parcels (C-afa9ffa993, C-ae204b1b36). No document places wells within the buildable area, so no protected resource governs the layout.
Cites C-ae204b1b36, C-afa9ffa993
Avoidable: yes
Offsets from wells, a pre-construction testing offer (C-5a262c9439) and hauled or tank-stored fire water (C-04a3f6e338) can remove the exposure. No documented limit on the aquifer or the water supply.
Cites C-5a262c9439, C-04a3f6e338
Pathway: standard
Well testing offer for private wells within 1,000 feet of pile driving (C-5a262c9439) and routine well or water-use registration if an on-site source is chosen. No contested approval is documented.
Cites C-5a262c9439
Impact likely: no
Wells are nearby but none is documented inside normal pile-driving offsets, and no protection area exists on the parcels (C-ae204b1b36, C-afa9ffa993). Solar pile driving and a hauled fire water supply are unlikely to affect neighbouring supplies. Testing is pathway and cost, not impact.
Cites C-ae204b1b36, C-afa9ffa993, C-5a262c9439
Supporting statements (4)
Each claim the row cites: the statement in the assessor's words, then the quote the engine found on the page.
C-04a3f6e338
There are no fire hydrants near the yard; the nearest pressurized water is in Carrollton, about 4 miles away.
Quoted from page 2
There are no fire hydrants
in the area; the nearest pressurized water is in Carrollton, about 4 miles away.
Battery Energy Storage System Fire Safety Narrative - Tamsin Ridge · DR-0014 · Page 2 · 2023-06-28
Source consultant_memo · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
Cited by EG-04 · Filed under AQ-03, EG-04
C-5a262c9439
Northfold should offer pre-construction testing of private wells within 1,000 feet of pile driving.
Quoted from page 2
Northfold should offer pre-construction testing of private
wells within 1,000 feet of pile driving.
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · Page 2 · 2023-06-05
Source consultant_memo · Claim type recommendation · Polarity neutral · Confidence high · Quote check exact, 100 of 100
C-ae204b1b36
Nearby residences and farmsteads rely on private water wells in the shale and sandstone aquifer.
Quoted from page 2
The nearby residences and farmsteads rely on
private water wells in the shale and sandstone aquifer.
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · Page 2 · 2023-06-05
Source consultant_memo · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
C-afa9ffa993
Ohio EPA source water protection mapping shows no drinking water source protection area within the parcels.
Quoted from page 2
Ohio EPA source water protection mapping shows no
drinking water source protection area within the parcels.
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · Page 2 · 2023-06-05
Source desktop_study · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
3 Permits and requirements
The requirements tied to the rows of this report, by level. Each quote from dated law is shown with its source, the version in force on the cut-off and the basis for it.
No requirement is tied to the rows of this report.
4 What is missing
The information requests the run raised for the rows of this report, by priority: what is missing, what follows from it, and whether it holds up the decision.
Low priority (3)
IR-e0cf50bd46 · Low priority
Provide the wellhead or source-water protection area map, sole-source aquifer map or state drinking-water program determination for the project area, or confirm none exists.
	Missing evidence
	Wellhead or source-water protection area map, sole-source aquifer map or state drinking-water program determination

	Consequence
	Groundwater and Water Supply is rated on partial evidence without it.

	Blocks the decision
	No

	Raised by
	completeness


IR-5b67c80546 · Low priority
Provide the private well survey, water well records or hydrogeologic desktop study for the project area, or confirm none exists.
	Missing evidence
	Private well survey, water well records or hydrogeologic desktop study

	Consequence
	Groundwater and Water Supply is rated on partial evidence without it.

	Blocks the decision
	No

	Raised by
	completeness


IR-6b1d8f8529 · Low priority
Provide the water supply plan, will-serve letter or water withdrawal permit (construction, panel washing, fire water) for the project area, or confirm none exists.
	Missing evidence
	Water supply plan, will-serve letter or water withdrawal permit (construction, panel washing, fire water)

	Consequence
	Groundwater and Water Supply is rated on partial evidence without it.

	Blocks the decision
	No

	Raised by
	completeness


5 Next steps and agencies
Next steps
Complete a private well survey and offer pre-construction testing within 1,000 feet of pile driving.
Set pile and trenching offsets from wells.
Confirm the construction and BESS fire water source (hauled, tanks or well) and any permit.
Agencies
Ohio EPA
Carroll County
SFM
6 Basis and limits
This report is a desk review of the documents quoted above, as the engine read them for an information cut-off of 2023-08-01.
It is not a field survey and not a modelled study: this review made no site visit and ran no acoustic, hydraulic or other model. Where the record is silent, the report says what is missing; it does not fill the gap.
Every statement, figure and quote is the engine's record as written. The headings and connecting words are fixed text of this room, the same in every report.
Documents quoted (2)
Battery Energy Storage System Fire Safety Narrative - Tamsin Ridge · DR-0014 · 2023-06-28 · page 2
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · 2023-06-05 · page 2
Versions and data hashes
As the engine and the exporter recorded them. Hashes are SHA-256.
	Information cut-off
	2023-08-01

	Engine version
	2.11.0

	Prompt version
	2026-11-08.1

	Rows pack
	rows.json sha256 a018ecd7e4703bc1

	Federal pack
	federal.json sha256 8841c555ff35d20b

	State pack
	oh.json sha256 d4780705e1f18d09

	Local pack
	oh_carroll_county.json sha256 905cd3308848e7e8

	Data room manifest
	0c7e80d0ad17d1e3ed4060b9702e5b1905060ae2896e9aad796a57b590005832

	Audit chain
	valid (19 events)

	QA status
	PASS_WITH_WARNINGS

	Rendered at
	2026-11-10T15:42:40+00:00

	Run record (annex)
	66fca2c4c0bfa90df1e8efb79c0d2f426536b41f50a6a9b6869dd85e4554fd50

	Exporter
	Prism/room/exporter 1.4.0
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