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Environmental Contamination: desk report
Tamsin Ridge Solar and Storage
This is a fictional demonstration project in which every organisation, person, parcel and finding is invented.
One row of the risk matrix, EN-04 Environmental Contamination, in the Environmental Resources section: what the record holds on it.
A desk review of the record as it stood: not a field survey and not a modelled study.
	Information cut-off
	2023-08-01

	Row in the matrix
	EN-04 Environmental Contamination


1 Finding
3  Resource is present, likely difficult to address
The engine shows this rating as 3
	The rule
	Code computed the rating from the assessor's inputs:
extent=core, avoidable=partly -> 3
Set by the rule

	Decision
	Released with flags

	The engine's reasons
	Uncited absence claims to weigh: C-0af700a251 (no record in the annex), C-2ff0fce9c8 (no record in the annex), C-e9a687c1a0
Agencies not in the register or the evidence: Ohio EPA

	Evidence state
	VERIFIED · field study or agency determination


The assessor's comments
Phase I ESA identifies REC 1: suspected brine and petroleum release at former tank battery on Parcel 5, with staining and stressed vegetation, where the substation and BESS yard are proposed. Limited Phase II recommended. Parcel 3 debris pile de minimis. Closed UST 0.8 mile south. East Block mine spoil noted.
Worst case
The same rule on the worst case gives no rating above the point.
	Scenario
	Phase II confirms brine and petroleum contamination across the proposed substation and BESS yard, needing agency-overseen remediation or relocation of the POI-adjacent facilities. Mine spoil on the East Block (not fully accessed) adds uncertainty.

	Step still pending
	Limited Phase II sampling at the Parcel 5 former tank battery

	Inputs in the worst case
	Extent core · Avoidable no · Pathway individual · Impact likely yes

	The rule on the worst case
	worst case (extent=core, avoidable=no -> 3) not above the point

	Claims that make it plausible
	C-fe98e6ae5a, C-faf2f8bc21, C-df8aadf77e, C-94c3a5488e, C-8dc8e662ac, C-421d66e93e


2 What the record shows
The five inputs
Present: yes
Phase I identifies REC 1, a suspected brine and petroleum release at the former tank battery on Parcel 5, with staining and stressed vegetation and no release report (C-fe98e6ae5a, C-b2025b56f8). Also a de minimis debris pile on Parcel 3 (C-02dc91fd44) and plugged wells (C-a7cffff0d2).
Cites C-fe98e6ae5a, C-b2025b56f8, C-02dc91fd44, C-a7cffff0d2
Extent: core
The REC lies where the substation and battery yard are proposed (C-faf2f8bc21, C-df8aadf77e), which is central buildable land.
Cites C-faf2f8bc21, C-df8aadf77e
Avoidable: partly
Substation and BESS siting on Parcel 5 is affected; avoidance would require resiting pending Phase II (C-46481122cf, C-94c3a5488e). The Parcel 3 debris is removable (C-1e239f0074). Other findings are closed or off site: the closed UST 0.8 mile south (C-fd18b09c16), the 2016 spill closed under ODNR oversight (C-b9b7baadd9).
Cites C-46481122cf, C-94c3a5488e, C-1e239f0074, C-fd18b09c16, C-b9b7baadd9
Pathway: standard
A limited Phase II is recommended at the Parcel 5 tank battery and debris removal on Parcel 3 (C-46481122cf, C-1e239f0074). No regulated remediation is documented yet; no NPL, CERCLA or brownfield sites are in the search distances (C-5c2ccff84a).
Cites C-46481122cf, C-1e239f0074, C-5c2ccff84a
Impact likely: yes
The REC lies on the proposed substation and BESS yard, and foundations are recommended only after Phase II sampling (C-faf2f8bc21, C-94c3a5488e). Brine chlorides can also limit revegetation.
Cites C-faf2f8bc21, C-94c3a5488e
Supporting statements (19)
Each claim the row cites: the statement in the assessor's words, then the quote the engine found on the page.
C-02dc91fd44
A farm debris pile with empty pesticide containers and scrap metal at the Strohl farmstead, Parcel 3, is a de minimis condition.
Quoted from page 1
a farm debris pile with empty
pesticide containers and scrap metal at the Strohl farmstead (Parcel 3), a de minimis condition
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 1 · 2023-01-27
Source consultant_memo · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
C-0497ffe228
No acid seeps were seen on the mine spoil.
Quoted from page 2
no acid seeps were seen.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 2 · 2023-01-27
Source field_study · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
C-061f16a94b
No title search for environmental liens or activity and use limitations was provided; a lien search is recommended once title commitments are issued.
Quoted from page 3
The user did not provide a title search for environmental liens or activity and use limitations
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 3 · 2023-01-27
Source consultant_memo · Claim type data_gap · Polarity neutral · Confidence high · Quote check exact, 100 of 100
Filed under EN-04, PE-05
C-1e239f0074
Removal of the debris pile and pesticide containers on Parcel 3 is recommended before construction.
Quoted from page 1
Removal of the debris pile and pesticide containers on Parcel 3 before construction.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 1 · 2023-01-27
Source consultant_memo · Claim type recommendation · Polarity neutral · Confidence high · Quote check exact, 100 of 100
C-2ace1138d8
No landfill or dump is listed on or next to the Property.
Quoted from page 2
No landfill or dump is listed on or next to the Property.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 2 · 2023-01-27
Source desktop_study · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
C-421d66e93e
Parts of the East Block woodlots were not accessible because of reclamation spoil and dense autumn olive.
Quoted from page 3
Parts of the woodlots in the East Block were not accessible
because of reclamation spoil and dense autumn olive.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 3 · 2023-01-27
Source consultant_memo · Claim type data_gap · Polarity neutral · Confidence high · Quote check exact, 100 of 100
Cited by EC-03 · Filed under EC-03, EN-04
C-46481122cf
A limited Phase II with soil and shallow groundwater sampling is recommended at the Parcel 5 former tank battery before the substation and BESS yard are sited there.
Quoted from page 1
A limited Phase II investigation (soil and shallow groundwater sampling for chlorides, petroleum hydrocarbons
and BTEX) at the former tank battery on Parcel 5
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 1 · 2023-01-27
Source consultant_memo · Claim type recommendation · Polarity neutral · Confidence high · Quote check exact, 100 of 100
Filed under AQ-03, EN-04
C-5c2ccff84a
No NPL, CERCLA, RCRA TSD facility or brownfield site is within the ASTM search distances.
Quoted from page 2
No National Priorities List (Superfund) site, CERCLA site, RCRA treatment, storage or disposal
 facility or brownfield is within the search distances.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 2 · 2023-01-27
Source desktop_study · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
C-8dc8e662ac
Surface mining occurred on the East Block in the 1950s and 1960s, reclaimed under the pre-1977 program; spoil can contain acid-forming material.
Quoted from page 2
surface mining on the East Block in the 1950s and 1960s, reclaimed under the pre-1977
program. Mine spoil can contain acid-forming material
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 2 · 2023-01-27
Source public_record · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
Filed under EN-02, EN-04
C-94c3a5488e
Substation and BESS foundations are recommended after Phase II environmental sampling at the former tank battery.
Quoted from page 3
after the Phase II
 environmental sampling at the former tank battery
Preliminary Geotechnical Engineering Report - Tamsin Ridge Solar and Storage Project · DR-0018 · Page 3 · 2023-05-15
Source consultant_memo · Claim type presence · Polarity presence · Confidence medium · Quote check exact, 100 of 100
C-a7cffff0d2
Two plugged and abandoned oil and gas wells are listed in ODNR records on Parcels 4 and 10.
Quoted from page 1
two plugged and abandoned oil and gas wells (Parcels 4 and 10) listed in
ODNR records
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 1 · 2023-01-27
Source public_record · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
Filed under EN-02, EN-04
C-a898a65a41
No environmental liens were found in the public records searched.
Quoted from page 3
Environmental liens: none found in the public records searched.
Commitment for Title Insurance No. ATA-23-0418 (Parcels 2, 5 and 9) · DR-0006 · Page 3 · 2023-04-18
Source public_record · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
C-b2025b56f8
Dark staining and stressed vegetation cover about 60 by 90 feet down-slope of the former tank battery on Parcel 5.
Quoted from page 1
Dark staining and stressed vegetation cover an area of about 60 by
90 feet down-slope of the former brine and crude oil tank battery
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 1 · 2023-01-27
Source field_study · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
C-b9b7baadd9
No HREC or CREC was identified; a 2016 brine spill was cleaned up under ODNR oversight and closed as de minimis.
Quoted from page 1
No HREC or CREC was identified. A reported 2016 brine spill at the same pad was cleaned up under ODNR
oversight and closed
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 1 · 2023-01-27
Source consultant_memo · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
C-df8aadf77e
Parcel 5 hosts the substation and BESS yard and has a 138 kV line, gathering pipeline and oil and gas lease.
Quoted from page 1
Substation, BESS yard; 138 kV line; gathering pipeline; oil and gas lease
Parcel Schedule 2023-07-14 · DR-0005 · Page 1 · 2023-07-14
Source developer_document · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
Cited by EN-01 · Filed under EN-01, PE-05
C-e571f3a9eb
Main power transformer holds about 14,000 gallons of mineral oil, so the substation needs an SPCC plan under 40 CFR Part 112.
Quoted from page 2
The main power transformer holds about 14,000 gallons of mineral oil, so the substation needs a Spill
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · Page 2 · 2023-06-05
Source consultant_memo · Claim type regulatory · Polarity presence · Confidence high · Quote check exact, 100 of 100
Cited by PE-03 · Filed under EN-04, PE-03
C-faf2f8bc21
The suspected Parcel 5 release is a REC lying where the substation and battery yard are proposed; brine chlorides can also limit revegetation.
Quoted from page 3
it
 lies where the substation and battery yard are proposed. Brine chlorides can also limit revegetation.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 3 · 2023-01-27
Source consultant_memo · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
Filed under EC-03, EN-01, EN-04
C-fd18b09c16
One closed leaking UST case is 0.8 mile south at a former filling station on State Route 43, down-gradient, closed with no further action.
Quoted from page 2
One closed leaking underground storage tank (UST) case is
0.8 mile south at a former filling station on State Route 43; it is down-gradient and closed with no further action.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 2 · 2023-01-27
Source desktop_study · Claim type presence · Polarity neutral · Confidence high · Quote check exact, 100 of 100
C-fe98e6ae5a
REC 1: a release of brine and petroleum to soil is suspected at the former tank battery site on Parcel 5, with no release report found.
Quoted from page 1
No release report for this area was found. A release of brine and petroleum to soil is
suspected.
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · Page 1 · 2023-01-27
Source consultant_memo · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
3 Permits and requirements
The requirements tied to the rows of this report, by level. Each quote from dated law is shown with its source, the version in force on the cut-off and the basis for it.
No requirement is tied to the rows of this report.
4 What is missing
The information requests the run raised for the rows of this report, by priority: what is missing, what follows from it, and whether it holds up the decision.
High priority (1)
IR-6b1aae03de · High priority
Provide the regulatory database screen (federal epa and state contaminated-site, release and tank lists) for the project area, or confirm none exists.
	Missing evidence
	Regulatory database screen (federal EPA and state contaminated-site, release and tank lists)

	Consequence
	Environmental Contamination is rated on partial evidence without it.

	Blocks the decision
	No

	Raised by
	completeness


5 Next steps and agencies
Next steps
Complete limited Phase II at Parcel 5 tank battery before fixing substation and BESS layout.
Remove Parcel 3 debris and pesticide containers before construction.
Obtain environmental lien and AUL search once title commitments are issued.
Agencies
Ohio EPA
ODNR
6 Basis and limits
This report is a desk review of the documents quoted above, as the engine read them for an information cut-off of 2023-08-01.
It is not a field survey and not a modelled study: this review made no site visit and ran no acoustic, hydraulic or other model. Where the record is silent, the report says what is missing; it does not fill the gap.
Every statement, figure and quote is the engine's record as written. The headings and connecting words are fixed text of this room, the same in every report.
Documents quoted (5)
Phase I Environmental Site Assessment - Tamsin Ridge Solar and Storage Project · DR-0012 · 2023-01-27 · pages 1, 2, 3
Preliminary Geotechnical Engineering Report - Tamsin Ridge Solar and Storage Project · DR-0018 · 2023-05-15 · page 3
Commitment for Title Insurance No. ATA-23-0418 (Parcels 2, 5 and 9) · DR-0006 · 2023-04-18 · page 3
Parcel Schedule 2023-07-14 · DR-0005 · 2023-07-14 · page 1
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · 2023-06-05 · page 2
Versions and data hashes
As the engine and the exporter recorded them. Hashes are SHA-256.
	Information cut-off
	2023-08-01

	Engine version
	2.11.0

	Prompt version
	2026-11-08.1

	Rows pack
	rows.json sha256 a018ecd7e4703bc1

	Federal pack
	federal.json sha256 8841c555ff35d20b

	State pack
	oh.json sha256 d4780705e1f18d09

	Local pack
	oh_carroll_county.json sha256 905cd3308848e7e8

	Data room manifest
	0c7e80d0ad17d1e3ed4060b9702e5b1905060ae2896e9aad796a57b590005832

	Audit chain
	valid (19 events)

	QA status
	PASS_WITH_WARNINGS

	Rendered at
	2026-11-10T15:42:40+00:00

	Run record (annex)
	66fca2c4c0bfa90df1e8efb79c0d2f426536b41f50a6a9b6869dd85e4554fd50

	Exporter
	Prism/room/exporter 1.4.0
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