
Tamsin Ridge Solar and Storage · Wetlands and waters report
Wetlands and waters report
Tamsin Ridge Solar and Storage
This is a fictional demonstration project in which every organisation, person, parcel and finding is invented.
Wetlands, streams, ponds, ditches and other surface waters in or crossing the study area, and whether they may be regulated waters.
A desk review of the record as it stood: not a field survey and not a modelled study.
	Information cut-off
	2023-08-01

	Row in the matrix
	AQ-01 Wetlands and Waterbodies


1 Finding
3  Resource is present, likely difficult to address
The engine shows this rating as 3
	The rule
	Code computed the rating from the assessor's inputs:
extent=core, avoidable=partly -> 3
Set by the rule

	Decision
	Released

	Evidence state
	VERIFIED · field study or agency determination


The assessor's comments
Sallow Creek, perennial, flows through the middle of the Project Area for about 6,850 linear feet. Five wetlands delineated, including Category 3 wetland W-3. Draft layout avoids wetlands; HDD planned for creek crossings and one ephemeral crossing under Nationwide Permit 14. ODNR recommends a 300-foot buffer on W-3.
Worst case
The same rule on the worst case gives no rating above the point.
	Scenario
	Final layout or HDD work affects W-3 or its 300-foot buffer, requiring Ohio EPA individual review and compensatory mitigation with a schedule effect of six months or more.

	Step still pending
	Preliminary jurisdictional determination and final design

	Inputs in the worst case
	Extent core · Avoidable partly · Pathway individual · Impact likely yes

	The rule on the worst case
	worst case (extent=core, avoidable=partly -> 3) not above the point

	Claims that make it plausible
	C-65f000df43, C-4a94b88b6a, C-3d096bbe0e, C-c98dca4336, C-8deff0ea95


2 What the record shows
The five inputs
Present: yes
Field delineation documents Sallow Creek, four tributaries and five wetlands including Category 3 wetland W-3 (C-8644116b06, C-a0386d398c, C-e5bfe1d5f5, C-3d096bbe0e). Upland cropland points without hydric indicators (C-cfe8567236) describe those points only and do not contradict the mapped features. Sallow Creek not being on the impaired list (C-846e2b0e13) concerns water quality, not presence.
Cites C-8644116b06, C-a0386d398c, C-e5bfe1d5f5, C-3d096bbe0e, C-cfe8567236, C-846e2b0e13
Extent: core
Perennial Sallow Creek flows north to south through the middle of the Project Area for about 6,850 linear feet, with its floodplain, W-3 and riparian forest (C-8644116b06, C-29b335e462, C-e10af45ca9, C-3d096bbe0e). It bisects the site, so collection and access routes must cross it.
Cites C-8644116b06, C-29b335e462, C-e10af45ca9, C-3d096bbe0e
Avoidable: partly
The May 8, 2023 draft layout avoids all five wetlands with ODNR buffers (C-13ca79b38e), but crossings are not avoidable: two HDD collection crossings of Sallow Creek and an S-4 ephemeral access road culvert (C-67f16faf2c, C-336bf30d1a, C-441acfa155). Avoidance of W-3 depends on final design.
Cites C-13ca79b38e, C-67f16faf2c, C-336bf30d1a, C-441acfa155
Pathway: standard
The only planned fill is about 40 linear feet (0.02 acre) of ephemeral channel under NWP 14 without pre-construction notification; HDD crossings need no permit absent frac-out (C-336bf30d1a, C-67f16faf2c). Ohio EPA general 401 coverage would apply (OH-401). Individual review arises only if W-3 is affected (C-4a94b88b6a).
Cites C-336bf30d1a, C-67f16faf2c, C-4a94b88b6a, C-8b50a6949e
Impact likely: yes
A culvert crossing of S-4 is planned and Sallow Creek will be bored beneath. A haul-route culvert at S-2 also needs load rating (C-336bf30d1a, C-67f16faf2c, C-fe62671132). Some physical effect on waters is likely even with avoidance of wetlands.
Cites C-336bf30d1a, C-67f16faf2c, C-fe62671132
Supporting statements (20)
Each claim the row cites: the statement in the assessor's words, then the quote the engine found on the page.
C-13ca79b38e
The May 8, 2023 draft layout avoids all five wetlands and keeps the ODNR buffers.
Quoted from page 3
The draft layout dated May 8, 2023 avoids all five wetlands and keeps the ODNR buffers.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 3 · 2023-05-22
Source developer_document · Claim type other · Polarity neutral · Confidence high · Quote check exact, 100 of 100
Cited by PE-03 · Filed under AQ-01, PE-02, PE-03
C-29b335e462
The SFHA follows Sallow Creek through the middle of the property.
Quoted from page 1
The special flood hazard area (SFHA) follows Sallow Creek through the middle of the property.
Standard Flood Hazard Determination - Tamsin Ridge Parcels 5, 9 and 10 · DR-0009 · Page 1 · 2023-03-15
Source agency_determination · Claim type presence · Polarity presence · Confidence medium · Quote check exact, 100 of 100
Cited by AQ-02
C-336bf30d1a
The S-4 access road crossing is the only planned fill: about 40 linear feet of ephemeral channel (0.02 acre) under NWP 14.
Quoted from page 3
about 40 linear feet of ephemeral channel (0.02 acre), within NWP 14 without pre-construction notification.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 3 · 2023-05-22
Source consultant_memo · Claim type extent · Polarity presence · Confidence high · Quote check exact, 100 of 100
Cited by EG-01, PE-03 · Filed under AQ-01, EG-01, PE-03
C-3d096bbe0e
Wetland W-3, a 4.1-acre forested wetland on the Sallow Creek floodplain in Parcel 9, is a Category 3 wetland (ORAM 66).
Quoted from page 1
Wetland W-3, a 4.1-acre forested wetland on the Sallow Creek floodplain in Parcel 9, scored 66 on ORAM and is a Category 3 wetland.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 1 · 2023-05-22
Source field_study · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
Filed under AQ-01, AQ-02
C-441acfa155
A USACE nationwide permit is expected for one access road crossing of an ephemeral stream.
Quoted from page 1
A U.S. Army Corps of Engineers nationwide permit is expected for one access road crossing of an ephemeral stream.
Tamsin Ridge Solar and Storage Project - Project Description · DR-0001 · Page 1 · 2023-06-12
Source developer_document · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
Cited by EC-01, PE-03 · Filed under AQ-01, PE-03
C-4a94b88b6a
Any impact to a Category 3 wetland needs Ohio EPA's individual review, and filling an isolated wetland needs an Ohio EPA permit.
Quoted from page 3
Filling an isolated wetland needs an Ohio EPA isolated wetland permit, and any impact to a Category 3 wetland
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 3 · 2023-05-22
Source consultant_memo · Claim type regulatory · Polarity presence · Confidence medium · Quote check exact, 100 of 100
Filed under AQ-01, PE-02, PE-03
C-65f000df43
If W-3 or its 300-foot buffer is affected, Ohio EPA individual review and compensatory mitigation would be needed, with a schedule effect of six months or more.
Quoted from page 3
Ohio EPA individual review and compensatory
mitigation would be needed, with a schedule effect of six months or more.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 3 · 2023-05-22
Source consultant_memo · Claim type schedule · Polarity presence · Confidence high · Quote check exact, 100 of 100
Filed under AQ-01, PE-02, PE-03
C-67f16faf2c
Two collection line crossings of Sallow Creek are planned as HDD bores of about 900 feet, needing no permit absent frac-out.
Quoted from page 3
The two collection line
crossings of Sallow Creek are planned as HDD bores of about 900 feet,
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 3 · 2023-05-22
Source consultant_memo · Claim type other · Polarity neutral · Confidence medium · Quote check exact, 100 of 100
Filed under AQ-01, PE-03
C-786ca1992e
Recommended to avoid all delineated wetlands with ODNR-expected buffers: 300 feet from W-3 and 120 feet from Category 1 and 2 wetlands.
Quoted from page 1
Avoid all delineated wetlands and keep the buffers ODNR expects for solar facilities: 300 feet from W-3
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 1 · 2023-05-22
Source consultant_memo · Claim type recommendation · Polarity neutral · Confidence high · Quote check exact, 100 of 100
Filed under AQ-01, EC-03
C-846e2b0e13
Sallow Creek is not on Ohio EPA's impaired waters list and no TMDL applies.
Quoted from page 1
Sallow Creek is not on Ohio EPA's list of impaired waters and no TMDL applies to it.
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · Page 1 · 2023-06-05
Source consultant_memo · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
Cited by EG-02 · Filed under AQ-01, EG-02
C-8644116b06
Sallow Creek, a perennial stream, flows through the middle of the Project Area for about 6,850 linear feet.
Quoted from page 1
Sallow Creek, a perennial stream, flows north to south through the middle of the Project Area for about 6,850
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 1 · 2023-05-22
Source field_study · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
C-8b50a6949e
Cross ephemeral stream S-4 with the East Block access road on a culvert under Nationwide Permit 14, with impacts expected below 0.1 acre.
Quoted from page 1
under Nationwide Permit 14; impacts are expected to be below 0.1 acre.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 1 · 2023-05-22
Source consultant_memo · Claim type recommendation · Polarity neutral · Confidence high · Quote check exact, 100 of 100
Cited by PE-03 · Filed under AQ-01, PE-02, PE-03
C-8deff0ea95
A preliminary jurisdictional determination should be requested before the OPSB application is filed.
Quoted from page 1
Request a preliminary jurisdictional determination before the OPSB application is filed.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 1 · 2023-05-22
Source consultant_memo · Claim type recommendation · Polarity neutral · Confidence high · Quote check exact, 100 of 100
Cited by PE-03 · Filed under AQ-01, PE-03
C-a0386d398c
Five wetlands totaling 9.8 acres were delineated in the Project Area: two PEM, one PSS and two PFO.
Quoted from page 1
Five wetlands totaling 9.8 acres were delineated: two palustrine emergent (PEM), one palustrine scrub-shrub
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 1 · 2023-05-22
Source field_study · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
C-c98dca4336
The Division recommends HDD for collection crossings of Sallow Creek and avoiding the Category 3 wetland with a 300-foot buffer.
Quoted from page 1
The Division recommends HDD for collection crossings of Sallow Creek and avoidance of
 the Category 3 wetland with a 300-foot buffer.
ODNR Environmental Review - Tamsin Ridge Solar and Storage Project (ODNR 23-0477) · DR-0011 · Page 1 · 2023-05-02
Source agency_determination · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
C-cfe8567236
Upland data points in the cropland showed no hydric indicators.
Quoted from page 2
Upland data points in the cropland showed no hydric indicators.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 2 · 2023-05-22
Source field_study · Claim type absence · Polarity absence · Confidence high · Quote check exact, 100 of 100
C-e10af45ca9
Riparian forest lines most of Sallow Creek's length.
Quoted from page 2
Riparian forest lines most of its length.
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 2 · 2023-05-22
Source field_study · Claim type presence · Polarity presence · Confidence medium · Quote check exact, 100 of 100
Cited by EC-03 · Filed under AQ-01, EC-03
C-e5bfe1d5f5
Four unnamed tributaries were delineated (two intermittent, two ephemeral), totaling 9,420 linear feet.
Quoted from page 1
Four unnamed tributaries were delineated: S-1 and S-2
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · Page 1 · 2023-05-22
Source field_study · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
C-ee75dcde7f
Sallow Creek supports a diverse fish assemblage, and no in-water work is recommended April 15 to June 30.
Quoted from page 1
Sallow Creek supports a diverse fish assemblage. No in-water work is recommended from
 April 15 to June 30.
ODNR Environmental Review - Tamsin Ridge Solar and Storage Project (ODNR 23-0477) · DR-0011 · Page 1 · 2023-05-02
Source agency_determination · Claim type presence · Polarity presence · Confidence high · Quote check exact, 100 of 100
Filed under AQ-01, EC-02
C-fe62671132
A stream designated S-2 is crossed by Dunmore Road, and Sallow Creek is crossed by Linnet Road.
Quoted from page 1
The Dunmore Road culvert at stream S-2 must be load-rated by the applicant's engineer before
 use.
Haul Route Review Comments - Tamsin Ridge Solar and Storage Project · DR-0029 · Page 1 · 2023-07-05
Source agency_determination · Claim type presence · Polarity presence · Confidence low · Quote check exact, 100 of 100
3 Permits and requirements
The requirements tied to the rows of this report, by level. Each quote from dated law is shown with its source, the version in force on the cut-off and the basis for it.
Federal (2)
Section 404 permit (Nationwide Permit, e.g. NWP 51, or Individual Permit)
F-CWA404 · U.S. Army Corps of Engineers (district by location)
	Applicability
	Conditional

	Instrument
	Clean Water Act Section 404 (33 U.S.C. 1344); 33 CFR Parts 320-332

	Trigger
	Fill or discharge in jurisdictional waters or wetlands (roads, crossings, grading).

	Description
	Regulates discharge of dredged or fill material into waters of the United States, including wetlands. Permit type depends on the area of impact and the activity. NWP 51 (land-based renewable energy) allows the loss of up to 1/2 acre of non-tidal waters, with pre-construction notification above 1/10 acre.

	Typical timeline
	NWP with a pre-construction notification: the permittee may presume the project qualifies unless the Corps responds within a 45-day period that starts on receipt of the notification (33 CFR 330.1(e)(1)); listed-species and historic-property clearances (see the Endangered Species Act and Section 106 rows) can hold authorization longer. Individual permit: decision target of 60 days after receipt of a complete application, subject to the exceptions in 33 CFR 325.2(d)(3). Typical: 2 to 4 months for an NWP with notification and 6 to 12 months or more for an individual permit (basis: practice, not stated in the sources).

	Version of the law on the cut-off
	33 CFR 330 as amended in 2022

	As of the cut-off
	As of the cut-off: The 16 NWPs reissued or issued in January 2021, including NWP 51 for land-based renewable energy, and the 32 general conditions took effect (86 FR 2744). (2021-03-15) A federal district court in Arizona (Pascua Yaqui Tribe v. EPA) vacated the 2020 Navigable Waters Protection Rule; from 2021-09-03 the agencies applied the pre-2015 regulatory definition of waters of the United States, read in light of Rapanos. (2021-08-30) The remaining 41 NWPs took effect under the same general conditions (86 FR 73522). (2022-02-25) A federal district court in Texas (Texas v. EPA, S.D. Tex.) preliminarily enjoined the 2023 rule in Texas and Idaho, where the agencies continued to apply the pre-2015 regulatory regime. (2023-03-19) The 2023 rule revising the definition of waters of the United States (88 FR 3004) took effect, but was not operative in some states because of litigation. (2023-03-20) A federal court in North Dakota enjoined the 2023 rule in the 24 plaintiff states, which include Virginia (West Virginia v. EPA). (2023-04-12) Sackett v. EPA narrowed the scope of waters of the United States. (2023-05-25) Announced by the cut-off, taking effect later (not applied): The 2021 NWPs, including NWP 51, expire; verification letters generally expire on the same date. (2026-03-14; announced 2021-01-13)

	Verification
	PACK_PENDING_QUALIFIED_REVIEW

	Source
	pack:federal

	In the permit matrix
	F-CWA404


Legal basis: 4 quotes from dated law
Quoted from the law, page 1
Except as provided in § 323.4 of this part, DA permits will be required for the discharge of dredged or fill material into waters of the United States. Certain discharges specified in 33 CFR part 330 are permitted by that regulation (“nationwide permits”).
Source 33CFR323 · page 1 · version 2023-08-01
Cited for requirement and trigger
In force from 2016-12-15 to 2026-10-07
eCFR versioner: 33 CFR part 323, same text on 2021-10-15, 2022-05-20, 2022-09-12, 2023-04-22, 2023-08-01 and on every amendment date between them; amendment dates 2016-12-15
May be cited on the cut-off date.
Quoted from the law, page 1
The permittee may presume that his project qualifies for the NWP unless he is otherwise notified by the DE within a 45-day period. The 45-day period starts on the date of receipt of the notification in the Corps district office and ends 45 calendar days later regardless of weekends or holidays.
Source 33CFR330 · page 1 · version 2023-08-01
Cited for timeline: NWP pre-construction notification
In force from 2022-03-21 to 2026-10-07
eCFR versioner: 33 CFR part 330, same text on 2022-05-20, 2022-09-12, 2023-04-22, 2023-08-01 and on every amendment date between them; amendment dates 2016-12-15, 2022-03-07, 2022-03-21
May be cited on the cut-off date.
Quoted from the law, page 1
District engineers will decide on all applications not later than 60 days after receipt of a complete application, unless (i) precluded as a matter of law or procedures required by law (see below)
Source 33CFR325 · page 1 · version 2023-08-01
Cited for timeline: individual permit decision target
In force from 2016-12-15 to 2025-07-02
eCFR versioner: 33 CFR part 325, same text on 2021-10-15, 2022-05-20, 2022-09-12, 2023-04-22, 2023-08-01 and on every amendment date between them; amendment dates 2016-12-15, 2025-07-03, 2025-07-15
May be cited on the cut-off date.
Quoted from the law, page 120
The discharge must not cause the loss of greater than 1⁄2-acre of non-tidal waters of the United States. This NWP does not authorize discharges of dredged or fill material into non-tidal wetlands adjacent to tidal waters. Notification: The permittee must submit a pre-construction notification to the district engineer prior to commencing the activity if the discharge results in the loss of greater than 1⁄10- acre of waters of the United States.
Source 86FR2744 · page 120 · version 2021-01-13
May be cited on the cut-off date.
Section 10 permit
F-RHA10 · U.S. Army Corps of Engineers
	Applicability
	Conditional

	Instrument
	Rivers and Harbors Act Section 10 (33 U.S.C. 403)

	Trigger
	Crossing or work in a navigable waterway.

	Description
	Work or structures in, over or under navigable waters of the United States.

	Typical timeline
	Same Corps process as Section 404: decision target of 60 days after receipt of a complete application, subject to the exceptions in 33 CFR 325.2(d)(3); a nationwide permit with a pre-construction notification follows the notification period described under the Section 404 row. Typical: 2 to 4 months for a nationwide permit with notification and 6 to 12 months or more for an individual permit (basis: practice, not stated in the sources).

	Version of the law on the cut-off
	33 CFR 320 as amended in 2022

	As of the cut-off
	Announced by the cut-off, taking effect later (not applied): The 2021 NWPs, which can authorize Section 10 work as well as Section 404 fill, expire. (2026-03-14; announced 2021-01-13)

	Verification
	PACK_PENDING_QUALIFIED_REVIEW

	Source
	pack:federal

	In the permit matrix
	F-RHA10


Legal basis: 3 quotes from dated law
Quoted from the law, page 1
DA permits are required under section 10 for structures and/or work in or affecting navigable waters of the United States except as otherwise provided in § 322.4 below.
Source 33CFR322 · page 1 · version 2023-08-01
Cited for requirement and trigger
In force from 2016-12-15 to 2026-10-07
eCFR versioner: 33 CFR part 322, same text on 2021-10-15, 2022-05-20, 2022-09-12, 2023-04-22, 2023-08-01 and on every amendment date between them; amendment dates 2016-12-15
May be cited on the cut-off date.
Quoted from the law, page 1
“Navigable waters of the United States” are defined in 33 CFR part 329. These are waters that are navigable in the traditional sense where permits are required for certain work or structures pursuant to Sections 9 and 10 of the Rivers and Harbors Act of 1899.
Source 33CFR320 · page 1 · version 2023-08-01
Cited for trigger: navigable waters of the United States
In force from 2022-03-21 to 2025-07-02
eCFR versioner: 33 CFR part 320, same text on 2022-05-20, 2022-09-12, 2023-04-22, 2023-08-01 and on every amendment date between them; amendment dates 2016-12-15, 2022-03-07, 2022-03-21, 2025-07-03
May be cited on the cut-off date.
Quoted from the law, page 1
District engineers will decide on all applications not later than 60 days after receipt of a complete application, unless (i) precluded as a matter of law or procedures required by law (see below)
Source 33CFR325 · page 1 · version 2023-08-01
Cited for timeline: decision target
In force from 2016-12-15 to 2025-07-02
eCFR versioner: 33 CFR part 325, same text on 2021-10-15, 2022-05-20, 2022-09-12, 2023-04-22, 2023-08-01 and on every amendment date between them; amendment dates 2016-12-15, 2025-07-03, 2025-07-15
May be cited on the cut-off date.
State (2)
Section 401 water quality certification (individual, or coverage under Ohio EPA's general certification of a Corps nationwide permit)
OH-401 · Ohio Environmental Protection Agency (Ohio EPA), Division of Surface Water (401 Water Quality Certification and Isolated Wetland Permitting Section)
	Applicability
	Conditional

	Instrument
	ORC 6111.03(O) and 6111.30; OAC Chapter 3745-32; Ohio EPA general 401 certification of the 2022 nationwide permits (2021-10-13)

	Trigger
	A federal license or permit (for example a Corps Section 404 permit) for an activity that may result in a discharge of dredged or fill material to a water of the state.

	Description
	Anyone who needs a federal license or permit, such as a Corps Section 404 permit, for an activity that may discharge dredged or fill material to a water of the state must obtain a 401 certification from Ohio EPA before starting. No separate application is needed for a Corps nationwide permit that Ohio EPA has certified, if the project meets the certification's terms and conditions. Ohio EPA's certification of the 2022 nationwide permits carries conditions; for example, Category 3 wetland impacts above 0.1 acre need an individual certification, although Ohio EPA can grant coverage to a project that does not meet a condition (a director's authorization). For the 2021 nationwide permits, listed in the dated events, the Corps notice states that Ohio's certification was waived; confirm the treatment with the Corps district. An individual application must include current Corps correspondence on the jurisdictional status of the waters.

	Typical timeline
	Individual certification: the application is due no later than 45 days after the Corps publishes its 404 public notice, and Ohio EPA acts within 180 days of a complete application. Nationwide permit with an Ohio EPA notification: work may proceed on Ohio EPA's written clearance, or once 45 calendar days have passed from Ohio EPA's receipt of the notification without a request for more information or an individual certification.

	As of the cut-off
	As of the cut-off: The Corps' notice for the 16 nationwide permits that took effect on this date (NWPs 12, 21, 29, 39, 40, 42, 43, 44, 48, 50, 51, 52, 55, 56, 57 and 58, which include NWP 51 for land-based renewable energy and NWP 57 for electric utility lines) states that Ohio's Section 401 certification was waived for them. (2021-03-15) The 41 nationwide permits reissued for 2022 (including NWP 14, linear transportation projects) took effect with Ohio EPA's general Section 401 certification, issued with conditions on 2021-10-13; they expire 2026-03-14. (2022-02-25)

	Verification
	PACK_PENDING_QUALIFIED_REVIEW

	Source
	pack:oh.json

	In the permit matrix
	OH-401


Legal basis: 8 quotes from dated law
Quoted from the law, page 5
Any applicant for a federal license or permit to conduct any activity which may result in a discharge of dredged or fill material to a water of the state shall apply for and obtain a 401 certification from Ohio EPA. (B) No person shall engage in an activity requiring a 401 certification prior to obtaining that certification from Ohio EPA.
Source OAC 3745 32 section 401 certification · page 5 · version 2023-08-01
In force from 2017-01-02 to 2024-07-19, section 3745-32-02
3745-32-02: version effective 2017-01-02; first change after it 2024-07-20 (Ohio EPA five-year review package for OAC 3745-32-01 to -04 (401 water quality certification; comment period 2023-11-03 to 2023-12-08); filing number not retrieved), from codes.ohio.gov version history in archive captures (confirmed_two_sources)
May be cited on the cut-off date.
Quoted from the law, page 6
If the federal permit sought is a nationwide permit, a regional permit, or a letter of permission issued by the corps and Ohio EPA has issued a certification for the federal permit, no further application is required to be submitted to Ohio EPA under this chapter provided that the project meets all of the terms and conditions
Source OAC 3745 32 section 401 certification · page 6 · version 2023-08-01
In force from 2017-01-02 to 2024-07-19, section 3745-32-03
3745-32-03: version effective 2017-01-02; first change after it 2024-07-20 (Ohio EPA five-year review package for OAC 3745-32-01 to -04; filing number not retrieved), from codes.ohio.gov version history in archive captures (confirmed_two_sources)
May be cited on the cut-off date.
Quoted from the law, page 7
The application shall be submitted no later than forty-five days after the publication of the corps 404 public notice, if applicable, and shall include the following: (a) Current and unexpired correspondence from the corps documenting the jurisdictional status of the waters located within the project area.
Source OAC 3745 32 section 401 certification · page 7 · version 2023-08-01
In force from 2017-01-02 to 2024-07-19, section 3745-32-03
3745-32-03: version effective 2017-01-02; first change after it 2024-07-20 (Ohio EPA five-year review package for OAC 3745-32-01 to -04; filing number not retrieved), from codes.ohio.gov version history in archive captures (confirmed_two_sources)
May be cited on the cut-off date.
Quoted from the law, page 39
(G) The director shall issue or deny a section 401 water quality certification not later than one hundred eighty days after the complete application for the certification is received.
Source ORC 6111 water pollution isolated wetlands 401 · page 39 · version 2023-08-01
In force from 2021-04-12 to 2026-10-03, section 6111.30
6111.30: version effective 2021-04-12, still the current version when the page map was checked (2026-10-03)
May be cited on the cut-off date.
Quoted from the law, page 5
D. DIRECTOR’S AUTHORIZATION 1. In accordance with the procedures outlined in Appendix A, Ohio EPA can grant coverage under this certification for any project that does not meet one or more of the terms and conditions for eligibility of this certification or where the district engineer has been granted authority to waive certain requirements.
Source OEPA 401 WQC for the 2022 Nationwide Permits 41 NWPs Ohio EPA ID 217512 · page 5 · version 2021-10-13
May be cited on the cut-off date.
Quoted from the law, page 6
a. They are notified in writing by Ohio EPA that the activity may proceed under the 401 WQC for the NWP; or b. 45 calendar days have passed from Ohio EPA’s receipt of the notification and the applicant has not received written notice from Ohio EPA that additional information is necessary or that an individual 401 WQC is required.
Source OEPA 401 WQC for the 2022 Nationwide Permits 41 NWPs Ohio EPA ID 217512 · page 6 · version 2021-10-13
May be cited on the cut-off date.
Quoted from the law, page 13
3. Individual 401 WQC is required for temporary or permanent impacts to category 3 wetlands that exceed 0.1 acres. Impacts to category 3 wetlands are only allowable for activities involving the repair, maintenance, replacement, or safety upgrades to existing infrastructure that meets the definition of public need.
Source OEPA 401 WQC for the 2022 Nationwide Permits 41 NWPs Ohio EPA ID 217512 · page 13 · version 2021-10-13
May be cited on the cut-off date.
Quoted from the law, page 4
The NWPs are not valid until the appropriate state agency certifies the discharge of dredged or fill material into waters of the U.S. does not violate state water quality standards or waives certification pursuant to 40 CFR § 121.9. The State of Ohio Section 401 Water Quality Certification has been waived for the 2021 NWPs.
Source Huntington District PN Nationwide Permits for Ohio 16 NWPs regional conditions · page 4 · version 2021-03-15
May be cited on the cut-off date.
State isolated wetland permit for filling an isolated wetland (Level 1 general permit, or Level 2 or Level 3 individual permit)
OH-IWP · Ohio Environmental Protection Agency (Ohio EPA), Division of Surface Water
	Applicability
	Conditional

	Instrument
	ORC 6111.02 to 6111.028; OAC 3745-1-50 to 3745-1-54; Ohio EPA Level 1 isolated wetland general permit (effective 2022-07-21)

	Trigger
	Filling an isolated wetland, meaning a wetland that is not subject to regulation under the federal Water Pollution Control Act.

	Description
	No one may fill an isolated wetland, meaning a wetland not subject to regulation under the federal Water Pollution Control Act, without an Ohio EPA isolated wetland permit. Review depends on wetland category and acreage. Level 1, a general permit: Category 1 or 2, one-half acre or less. Level 2, an individual permit: Category 1 over one-half acre, or Category 2 over one-half acre up to three acres. Level 3, an individual permit: Category 2 over three acres, or any Category 3. Ohio EPA lists review periods of 30, 90 and 180 days, public notice for Levels 2 and 3, and a mandatory hearing for Category 3. A Level 1 notice needs an ORAM 5.0 form for each wetland and a Corps determination that the wetlands are not waters of the United States; a preliminary jurisdictional determination treats all wetlands as federal.

	Typical timeline
	Ohio EPA review periods: 30 days for a Level 1 general permit, 90 days for a Level 2 individual permit and 180 days for a Level 3 individual permit, as listed on Ohio EPA's program page.

	Version of the law on the cut-off
	As in force from 2023-05-17 (the library text)

	As of the cut-off
	As of the cut-off: Ohio EPA's Level 1 isolated wetland general permit (Category 1 and 2 wetlands, one-half acre or less) took effect and runs to 2027-07-21; it was in force on the cut-off. (2022-07-21) Sackett v. EPA held that the Clean Water Act reaches an adjacent wetland only if it has a continuous surface connection to a relatively permanent water of the United States, so more wetlands can fall outside federal jurisdiction and count as isolated under ORC 6111.02. By 2023-07-20 the federal agencies' implementation page said they would interpret waters of the United States consistent with the decision. (2023-05-25)

	Verification
	PACK_PENDING_QUALIFIED_REVIEW

	Source
	pack:oh.json

	In the permit matrix
	OH-IWP


Legal basis: 8 quotes from dated law
Quoted from the law, page 21
No person shall engage in the filling of an isolated wetland unless authorized to do so by a general or individual state isolated wetland permit.
Source ORC 6111 water pollution isolated wetlands 401 · page 21 · version 2023-08-01
In force from 2001-07-17 to 2026-10-03, section 6111.021
6111.021: version effective 2001-07-17, still the current version when the page map was checked (2026-10-03)
May be cited on the cut-off date.
Quoted from the law, page 2
(F) "Isolated wetland" means a wetland that is not subject to regulation under the Federal Water Pollution Control Act.
Source ORC 6111 water pollution isolated wetlands 401 · page 2 · version 2023-08-01
In force from 2015-09-29 to 2026-10-03, section 6111.02
6111.02: version effective 2015-09-29, still the current version when the page map was checked (2026-10-03)
May be cited on the cut-off date.
Quoted from the law, page 2
including a determination from the U.S. Army Corps of Engineers that the wetlands proposed to be covered by this general permit are not Waters of the United States and not subject to Section 404 of the Clean Water Act; 3) A completed Ohio Rapid Assessment Method (ORAM 5.0) wetland categorization form for each isolated wetland on the project site.
Source OEPA Level 1 Isolated Wetland General Permit 228038 · page 2 · version 2022-07-21
May be cited on the cut-off date.
Quoted from the law, page 22
A proposed filling of a category 1 or a category 2 isolated wetland of one-half acre or less shall require a general state isolated wetland permit and be subject to level one review requirements established under division (B) of this section.
Source ORC 6111 water pollution isolated wetlands 401 · page 22 · version 2023-08-01
In force from 2012-09-05 to 2026-10-03, section 6111.022
6111.022: version effective 2012-09-05, still the current version when the page map was checked (2026-10-03)
May be cited on the cut-off date.
Quoted from the law, page 24
A proposed filling of a category 1 isolated wetland of greater than one-half acre or the proposed filling of a category 2 isolated wetland of greater than one-half acre, but less than or equal to three acres shall require an individual state isolated wetland permit and be subject to level two review requirements established under division (B) of this section.
Source ORC 6111 water pollution isolated wetlands 401 · page 24 · version 2023-08-01
In force from 2012-09-05 to 2026-10-03, section 6111.023
6111.023: version effective 2012-09-05, still the current version when the page map was checked (2026-10-03)
May be cited on the cut-off date.
Quoted from the law, page 28
A proposed filling of a category 2 isolated wetland of greater than three acres or a category 3 isolated wetland shall require an individual state isolated wetland permit and be subject to level three review requirements established under division (B) of this section.
Source ORC 6111 water pollution isolated wetlands 401 · page 28 · version 2023-08-01
In force from 2012-09-05 to 2026-10-03, section 6111.024
6111.024: version effective 2012-09-05, still the current version when the page map was checked (2026-10-03)
May be cited on the cut-off date.
Quoted from the law, page 1
30 days* General Permit Level 1 1 more than 0.5 acres Yes No 90 days* Individual Level 2 Isolated Wetland Permit Level 2 2 more than 0.5 acres but less than or equal to 3 acres 2 more than 3 acres Yes No 180 days* Individual Level 3 Isolated Wetland Permit Level 3 3 any size Yes Yes
Source OEPA 401 Water Quality Certification and Isolated Wetland Permits web page · page 1 · version 2023-05-17
May be cited on the cut-off date.
Quoted from the law, page 1
recorded in a final jurisdictional determination (JD) which is sent to the entity requesting the JD and to Ohio EPA. PLEASE NOTE: When the applicant requests, and the U.S. Army Corps of Engineers issues, a preliminary JD, all wetlands on the proposed site are assumed to be waters of the U.S. and will not be declared isolated.
Source OEPA 401 Water Quality Certification and Isolated Wetland Permits web page · page 1 · version 2023-05-17
May be cited on the cut-off date.
4 What is missing
The information requests the run raised for the rows of this report, by priority: what is missing, what follows from it, and whether it holds up the decision.
High priority (2)
IR-a33eeefca9 · High priority
Provide the usace jurisdictional determination or agency waters correspondence for the project area, or confirm none exists.
	Missing evidence
	USACE jurisdictional determination or agency waters correspondence

	Consequence
	Wetlands and Waterbodies is rated on partial evidence without it.

	Blocks the decision
	No

	Raised by
	completeness


IR-9f6495626a · High priority
Provide the desktop nwi/nhd water review or constraints mapping for the project area, or confirm none exists.
	Missing evidence
	Desktop NWI/NHD water review or constraints mapping

	Consequence
	Wetlands and Waterbodies is rated on partial evidence without it.

	Blocks the decision
	No

	Raised by
	completeness


5 Next steps and agencies
Next steps
Request preliminary jurisdictional determination before OPSB filing.
Keep layout out of W-3 and its 300-foot buffer; use HDD at Sallow Creek.
Obtain NWP 14 and Ohio EPA 401 coverage; observe the April 15 to June 30 in-water window.
Agencies
USACE Huntington District
Ohio EPA
ODNR
6 Basis and limits
This report is a desk review of the documents quoted above, as the engine read them for an information cut-off of 2023-08-01.
It is not a field survey and not a modelled study: this review made no site visit and ran no acoustic, hydraulic or other model. Where the record is silent, the report says what is missing; it does not fill the gap.
Every statement, figure and quote is the engine's record as written. The headings and connecting words are fixed text of this room, the same in every report.
Documents quoted (6)
Wetland and Stream Delineation Report - Tamsin Ridge Solar and Storage Project · DR-0013 · 2023-05-22 · pages 1, 2, 3
Standard Flood Hazard Determination - Tamsin Ridge Parcels 5, 9 and 10 · DR-0009 · 2023-03-15 · page 1
Tamsin Ridge Solar and Storage Project - Project Description · DR-0001 · 2023-06-12 · page 1
Stormwater, Floodplain and Drainage Memo - Tamsin Ridge Solar and Storage Project · DR-0019 · 2023-06-05 · page 1
ODNR Environmental Review - Tamsin Ridge Solar and Storage Project (ODNR 23-0477) · DR-0011 · 2023-05-02 · page 1
Haul Route Review Comments - Tamsin Ridge Solar and Storage Project · DR-0029 · 2023-07-05 · page 1
Versions and data hashes
As the engine and the exporter recorded them. Hashes are SHA-256.
	Information cut-off
	2023-08-01

	Engine version
	2.11.0

	Prompt version
	2026-11-08.1

	Rows pack
	rows.json sha256 a018ecd7e4703bc1

	Federal pack
	federal.json sha256 8841c555ff35d20b

	State pack
	oh.json sha256 d4780705e1f18d09

	Local pack
	oh_carroll_county.json sha256 905cd3308848e7e8

	Data room manifest
	0c7e80d0ad17d1e3ed4060b9702e5b1905060ae2896e9aad796a57b590005832

	Audit chain
	valid (19 events)

	QA status
	PASS_WITH_WARNINGS

	Rendered at
	2026-11-10T15:42:40+00:00

	Run record (annex)
	66fca2c4c0bfa90df1e8efb79c0d2f426536b41f50a6a9b6869dd85e4554fd50

	Legal source index
	6974703924a38a8e90717222e31e444b8e540aca9b6cec809ad4ddc5b0691ca9

	Exporter
	Prism/room/exporter 1.4.0
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